Spinneybeck introduced full grain, aniline dyed Italian leathers to North America in 1962. With more than 1,000 colorways in over 30 families of leather upholstery as well as architectural products, Spinneybeck is recognized as a leading provider of high-quality leather to architects and interior designers. Over the decades, the company has evolved from a supplier of full grain, aniline dyed Italian leather for upholstery and aircraft interiors to a manufacturer of pioneering, architectural products made from natural materials to cover the floor, walls, and everywhere in between. In addition, Spinneybeck’s work with industry design leaders in the fields of sculpture, architecture, interior design, and textiles has generated inventive leathers, color work, patterned wall tiles, drawer pulls, and sculpted wall systems. Regardless of the application, Spinneybeck has consistently held the same high standards for quality, originative products, environmental practices, and customer service.

SECTION 097219

LEATHER WALL COVERINGS

1. GENERAL
	* + 1. SUMMARY
				1. Provide architectural leather products and accessories of the following types:

Leather wall panels.

* + - * 1. Related Sections: Coordinate with the following as applicable:

Section 092116 - Gypsum Board Assemblies for substrate.

* + - 1. SUBMITTALS
				1. Product Data: Submit manufacturer's literature including product characteristics and accessories.
				2. Shop Drawings: Submit diagram showing layout of pattern and configuration, including details of perimeter conditions and mounting.
				3. Verification Samples: Submit samples of materials selected for use to verify color and finish.
			2. QUALITY ASSURANCE
				1. Manufacturer: Minimum of 5 years experience manufacturing similar products.
				2. Installer: Minimum of 2 years experience installing similar products.
				3. Field Measurements: To the greatest extent practical, take field measurements prior to fabrication.
			3. DELIVERY, STORAGE AND HANDLING
				1. Deliver materials and products in unopened factory labeled packages. Store and handle in strict compliance with manufacturer's instructions and recommendations.
1. PRODUCTS
	* + 1. MANUFACTURER
				1. Basis-of-Design Manufacturer: Spinneybeck, 425 CrossPoint Parkway, Getzville, NY 14068. Tel 800.482.7777, 716.446.2380. Fax 716.446.2396. sales@spinneybeck.com, www.spinneybeck.com.
			2. WALL PANELS
				1. Basis of Design: ARO Plank 1 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-1; two distinct half round modules that are composed of leather-wrapped extruded foam and available in four standard configurations.

Content: European cowhide, extruded foam, and plywood.

Plank A Width: 4-1/4 inches (10.8 cm).

Plank B Width: 2-1/4 inches (5.7 cm).

Plank C Width: 6-1/4 inches (15.9 cm).

Plank D Width: 8-1/4 inches (21 cm).

Plank E Width: 10-1/4 inches (26 cm).

Plank F Width: 1’-0 1/4” (31.1 cm).

Configuration: [Plank 1.1: A] [Plank 1.2: B] [Plank 1.3: AAABB] [ARO Plank 1.4: DFBEAECBACADACFBCAECBACADACD] [ARO Plank 1.5: ABABBBABBB] [ARO Plank 1.6: EECFEBEACFEABCEBFABAAACEC] [ ARO Plank 1.7: BACDEFFEDCAB] [ARO Plank 1.8: BFBD] [\_\_\_\_\_].

Length: \_\_\_\_\_\_ (9’-0” maximum standard length).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Seam: [Top Stitch] [Blind Stitch].

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 2 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-2; two distinct faceted modules with angled edges.

Content: European cowhide, PET substrate, and plywood.

Plank A Width: 5 inches (12.7 cm).

Plank B Width: 3 inches (7.6 cm).

Configuration: [Plank 2.1: A] [Plank 2.2: AA with every other plank rotated 180 degrees] [Plank 2.3: B] [Plank 2.4: BB with every other plank rotated 180 degrees] [Plank 2.5: AAABB] [\_\_\_\_\_].

Length: \_\_\_\_\_\_ (9’-0” maximum standard length).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Seam: [Top Stitch] [Blind Stitch].

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 3 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-3; one faceted module which is rotated and repeated.

Content: European cowhide, PET substrate, and plywood.

Plank Top Width: 5 inches (12.7 cm).

Plank Bottom Width: 3 inches (7.6 cm).

Configuration: [Plank 3: AA with every other plank rotated 180 degrees] [\_\_\_\_\_].

Length: \_\_\_\_\_\_ (9’-0” maximum standard length).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Seam: [Top Stitch] [Blind Stitch].

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 4 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-4; flat planks are accented by ribs, creating a striped, corrugated effect.

Content: European cowhide, PET substrate, and plywood.

Plank A Width: 1 foot 6 inches (45.7 cm).

Plank B Width: 9 inches (22.9 cm).

Rib Width: 1-1/4 inches (3.2 cm).

Configuration: [Plank 4.1: AC] [Plank 4.2: ACACCACCC] [Plank 4.3: BC] [Plank 4.4: BCBCCBCCC] [\_\_\_\_\_].

Length: \_\_\_\_\_\_ (9’-0” maximum standard length).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Seam: [Machine stitched at random intervals] [\_\_\_\_\_].

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 5 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-5; three chamfered modules, set at varying depths to cast compelling, evolving shadows.

Content: European cowhide, PET substrate, and plywood.

Plank A Width: 3.5” (9 cm).

Plank B Width: 2” (5 cm).

Plank C Width: 2” (5 cm).

Plank A Length: 7’-9” (236 cm).

Plank B Length: 5’-2” (157 cm).

Plank C Length: 2’-7” (157 cm).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 6 by Spinneybeck, www.spinneybeck.com/aro-plank-6; two distinct half round modules that are composed of leather-wrapped extruded foam and available in four standard configurations.

Content: European Cowhide, Acoustic Substrate.

Module A Width: 4 1/4 in (10.8 cm).

Module B Width: 4 1/4 in (10.8 cm).

Module C Width: 4 1/4 in (10.8 cm).

Module D Width: 2 1/4 in (5.7 cm).

Module E Width: 2 1/4 in (5.7 cm).

Configuration: [ARO Plank 6.1: ACCBCC] [ARO Plank 6.2: DEEEEEED\*EEEEEE (\* indicates plank rotated 180 degrees)] [ARO Plank 6.3: DEEDEEEEEED\*EED\*EEEEE (\* indicates plank rotated 180 degrees)] [ARO Plank 6.4: CCDCCD\* (\* indicates plank rotated 180 degrees)] [ARO Plank 6.5: AEEBEE] [ARO Plank 6.6: CBCEEB\*CA\*EECB\*CDEACCD\*ECA\*CEECACEE (\* indicates plank rotated 180 degrees)] [\_\_\_ (insert custom configuration)].

Length: \_\_\_\_\_\_ (9’-0” maximum standard length).

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Seam: [Blind Stitch].

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 7 by Spinneybeck, [www.spinneybeck.com](http://www.spinneybeck.com)/aro-plank-7

Content: European Cowhide, Akustika 10.

Module A Size: 5’-6” (167.6 cm) x 3 1/2” (8.9 cm) x 1 1/4” (3.2 cm).

Module B Size: 2’-7” (78.7 cm) x 2” (5.1 cm) x 1 1/4” (3.2 cm).

Module C Size: 2” (5.1 cm) x 2” (5.1 cm) x 3/4” (1.9 cm).

Configuration: [Manufacturer’s Standard Configuration] [\_\_\_ (insert custom configuration)].

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Attachment Method: Interlock Mounting System.

* + - * 1. Basis of Design: ARO Plank 8 by Spinneybeck, www.spinneybeck.com/aro-plank-8; two distinct half round modules that are composed of leather-wrapped extruded foam and available in four standard configurations.

Content: European Cowhide, Acoustic Substrate.

Module A Size: 2’-9” (83.8 cm) x 3 1/2” (8.9 cm) x 1 1/4” (3.2 cm).

Module B Size: 2’-9” (83.8 cm) x 2” (5.1 cm) x 3/4” (1.9 cm).

Module C Size: 3’-3 1/2” (100.3 cm) x 2” (5.1 cm) x 3/4” (1.9 cm)

Module D Size: 2’-2 1/2” (67.3 cm) x 2” (5.1 cm) x 3/4” (1.9 cm)

Module E Size: 6 1/2” (16.5 cm) x 2” (5.1 cm) x 3/4” (1.9 cm).

Configuration: [ARO Plank 8.1: A + B] [ARO Plank 8.2: A, D, E] [ARO Plank 8.3: A, C, D] [\_\_\_ (insert custom configuration)].

Orientation: [Vertical] [Horizontal].

Leather Type: [Andes (AD)] [Alaska (AL)] [Antique (AQ)] [Acqua (AU)] [Cascia (CA)] [Copenhagen (CO)] [Cervo (CV)] [Derby (DE)] [Ducale (DL)] [Distressed (DT)] [Ducale Velour (DV)] [Espana (ES)] [Embossed Tipped (ET)] [Forte (FE)] [Hand Tipped (HT)] [Lucca (LC)] [Lucente (LU)] [Maremma (MM)] [Portofino (PT)] [Riva (RA)] [Rugata (RU)] [Sabrina (SA)] [Saddle (SL)] [Umbria (UM)] [Volo (VO)] [Velluto Pelle (VP)] [Vicenza (VZ)].

Color: [\_\_\_\_\_\_\_\_] [As selected from manufacturer’s full range.]

Thread Color: [Matching primary leather colors] [\_\_\_\_\_].

Attachment Method: Interlock Mounting System.

1. EXECUTION
	* + 1. EXAMINATION
				1. Examine substrates for compliance with requirements for installation tolerances and other conditions affecting performance. Proceed with installation only after unsatisfactory conditions have been corrected.
			2. INSTALLATION
				1. Install products in strict accordance with manufacturer’s instructions and approved submittals.

Clean substrate of dirt and bond breaking substances prior to beginning installation.

Acclimatize leather at the installation site for a minimum of 48 hours prior to installation.

Follow manufacturer’s recommendations for adhesives and mounting devices.

Replace damaged or defaced products prior to Substantial Completion.

* + - 1. CLEANING
				1. Clean surfaces to remove soiling, stains, dust, and dirt using materials acceptable to manufacturer.
				2. Leave installation area clean, free of residue and debris resulting from work of this Section.

END OF SECTION